{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"merged":[[0,0,0,7],[20,0,20,1],[21,0,21,7]],"flags":["formulas_cached_only"]}
["房地产交易中心空调维修保养"]
["序号","项目名称","维修内容及要求","单位","数量","单价\n（元）","合价\n（元）","备注"]
[1,"制冷剂R22","制冷剂充注，制冷剂充注后需满足现场及甲方要求","公斤",45,null,{"v":0,"d":"0.00"},"约克原厂，需提供原厂证明材料"]
[2,"冷冻油","冷冻油更换，冷冻油更换后需满足现场及甲方要求","升",60,null,{"v":0,"d":"0.00"},"约克原厂，需提供原厂证明材料"]
[3,"油燥过滤器更换","拆除、更换，油燥过滤器更换后需满足现场及甲方要求","只",1,null,{"v":0,"d":"0.00"},"约克原厂，需提供原厂证明材料"]
[4,"干燥过滤器更换","拆除、更换，干燥过滤器更换后需满足现场及甲方要求","只",1,null,{"v":0,"d":"0.00"},"约克原厂，需提供原厂证明材料"]
[5,"引射过滤器更换","拆除、更换，引射过滤器更换后需满足现场及甲方要求","只",2,null,{"v":0,"d":"0.00"},"约克原厂，需提供原厂证明材料"]
[6,"冷凝器清洗养护","物理通炮，药水循环清洗，冷凝器清洗养护后需满足现场及甲方要求","只",1,null,{"v":0,"d":"0.00"}]
[7,"蒸发器清洗养护","物理通炮，药水循环清洗，蒸发器清洗养护后需满足现场及甲方要求","只",1,null,{"v":0,"d":"0.00"}]
[8,"2#机组滑阀传感器更换","拆除、更换，2#机组滑阀传感器更换后需满足现场及甲方要求","个",1,null,{"v":0,"d":"0.00"}]
[9,"1#机组显示器故障","检查、维修，1#机组显示器维修后需满足现场及甲方要求","台",1,null,{"v":0,"d":"0.00"}]
[10,"冷冻泵维修","型号：ELF250M-4 55KW、部位名称：3#、4#泵、现场症状：压力过高跳闸，冷冻泵维修后需满足现场及甲方要求\n","组",2,null,{"v":0,"d":"0.00"}]
[11,"冷却泵维修","型号：ELF280S-4 75KW、部位名称：7#、8#泵、现场症状：压力过大，冷却泵维修后需满足现场及甲方要求\n","组",2,null,{"v":0,"d":"0.00"}]
[12,"风机维修","型号：Y2132S-4 5.5KW 1440r/min、部位名称：裙一楼4#风机、现场症状：异响，风机维修后需满足现场及甲方要求\n","项",1,null,{"v":0,"d":"0.00"}]
[13,"新风机维修","部位名称：一楼东、西侧、现场症状：电气故障（西侧电流过大易保护停机），新风机维修后需满足现场及甲方要求\n","台",2,null,{"v":0,"d":"0.00"}]
[14,"接触器维修","部位名称：裙二楼13#、现场症状：接触器故障，接触器维修后需满足现场及甲方要求\n","项",1,null,{"v":0,"d":"0.00"}]
[15,"电机维修","部位名称：裙二楼10#、11#、13#、36#、30#、34#、39#电机、现场症状：异响，电机维修后需满足现场及甲方要求\n","台",7,null,{"v":0,"d":"0.00"}]
[16,"DN40减压阀更换","阀门拆除、更换，含配套保温拆除、恢复、附件等，DN40减压阀更换后需满足现场及甲方要求\n","个",1,null,{"v":0,"d":"0.00"}]
[17,"压力表更换","拆除、更换，压力表更换后需满足现场及甲方要求\n","套",6,null,{"v":0,"d":"0.00"}]
[18,"压力控制器更换","拆除、更换，压力控制器更换后需满足现场及甲方要求\n","个",2,null,{"v":0,"d":"0.00"}]
["合计",{"$nulls":5},{"v":0,"d":"0.00"}]
["1、以上报价为固定全费用单价，包含人工费、材料费、机械费、管理费、利润、规费、税金（按9%增值税专票考虑，实际开具的增值税专票税率低于9%部分的差额，招标人在结算时予以扣除）等一切费用。\n2、具体工作内容及工程量由建设单位确认。"]